Quick Start for Simple Serial Interface to NDI Tracking Systems

1. **Turn on Linux machine and log in.**
2. **Open a terminal, issue the following command**

**> cd ~/github/tracker-serial-interface**

|  |  |
| --- | --- |
| **Stream mode: capture frames (all tools) at full speed** | **> ./track\_server** |
| **Manual mode: capture one frame (all tools) when Enter is pressed** | **> ./track\_server -m** |
| **Listen mode: monitor serial port for capture request packets** | **> ./track\_server -l** |